|  |  |
| --- | --- |
| **Date** | 4 February 2019 |
| **Location** | Kelapa Gading Mall Station. |
| **Test Agenda** | Test PA,PID,PHP,VOIP Screen |
| **Testing Condition** | |
| 1. Testing PA Live and DVA on Kelapa Gading Mall 2. Testing VOIP+PHP on Kelapa Gading Mall. 3. Testing VOIP Status Call on Kelapa Gading Mall. 4. Testing PID on Kelapa Gading Mall. 5. Testing Microphone Status on Kelapa Gading Mall. | |
| **Testing Item** | |
| 1. Get All Status PA 2. Selecting zone and Initiate PA Live 3. Selecting zone and Initiate DVA Live 4. Testing VOIP via PHP 5. Testing VOIP to VOIP Call 6. Testing Status Microphone Idle,and Fault | |
| **Result** | |
| 1. This is status realtime when the driver’s and PA devices Available.     Figure 1. Status Realtime PA     1. We’re selecting one zone on Scr room only for some testing because we worried another employee activities, Testing PA Live     Figure 2. Selecting Zone PA and initiate PA Live via Microphone   1. We’re selecting one zone on Scr room only for some testing because we worried another employee activities, Testing PA Pre recorded DVA     Figure 3. Selecting Zone PA and initiate PA from Pre defined   1. Testing PHP via VOIP from platform to SCR room     Figure 4. Testing PHP VOIP from Platform to SCR room   1. Testing VOIP Call from PAO room to SCR Room     Figure 5. Testing VOIP from PAO room to SCR room   1. Testing Status Microphone     Figure 6. Testing Status microphone Idle    Figure 7. Testing Status microphone Fault   1. Testing PID, the text before is testing and after send to pid via HMI that’s become ‘Door Closing’     Figure 8. Testing PID Text to all zone, and this is Platform zone | |